|  |  |
| --- | --- |
| **Model:** | 9000CDT |
| **Version:** | V1.50 |
| **Issue date:**  **Type:** | 12th Dec 2023  Public |

|  |  |
| --- | --- |
| **New Features** |  |
|  |  |

|  |  |
| --- | --- |
| **Improvement** |  |
| * Fixes a bug when displaying the total time of a CD |  |

|  |  |
| --- | --- |
| **Additional information** |  |
| Firmware update instructions.  1. Turn off the power supply to the device (rear panel mains switch)  2. Install the update file on a FAT32 formatted USB drive (folder name must be '9000CDT' and contents should include 9000CDT.bin)  3. Insert the USB drive to the 'UPDATE' USB socket on the rear panel of the device.  4. Push and hold front panel standby button.  5. Turn on the power supply to the device (rear panel mains switch) while continuing to hold the standby button.  6. Release the standby button and the display will show 'upgrade processing'.  7. Allow the device to apply the software update. This may take a few minutes.  8. When update is complete, the device is ready to use. | |

|  |  |
| --- | --- |
| **Change history** |  |

V1.49

Improve backlight brightness

V1.46

First release version